Part A)

2.

Maximum electrical frequency can be found from the maximum speed which is 14000 rpm which is equal to 1466 rad/sec.

Then, we can modulate our signal with the ten times of the frequency of the signal. So our switching frequency of the inverter can be 2333 Hz.